\chapter{Logikanalysator}
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\section{Teilaufgabe1: Messen von $f_{hsync}$ und $f_{vsync}$ }
Bei dieser Teilaufgabe mussten wir horizontale Synchronisationsfrequenz $f_{hsync}$ und die vertikale Synchronisationsfrequenz $f_{vsync}$ mittels geeignete Modi bestimmem. Dabei war gegeben, dass $f_{hsync}$ per Timing-Mode und $f_{vsync}$ per State-Mode gemessen wird.

\subsection{$f_{hsync}$}
%bsp1_hsync_trigger.jpg
%bsp1_hsync_wave.jpg

\subsection{$f_{hsync}$}
%bsp1_vsync_trigger.jpg
%bsp1_vsync_wave.jpg


%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\section{Teilaufgabe2: Farbe des Pixels (317,148)}
%bsp2_trigger.jpg
%bsp2_wave.jpg


%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\section{Teilaufgabe3: Hintergrund und Objektkante}
%bsp3a_trigger.jpg
%bsp3a_wave.jpg
%bsp3b_trigger.jpg
%bsp3b_wave.jpg


%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\section{Teilaufgabe4: Hsync-FSM}
%bsp4_fsm1.jpg
%bsp4_fsm2.jpg


%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\section{Ergebnisse}
\begin{itemize}
\item Frequenz HSYNC = 29.458$\mu$s == ??? Hz
\item Frequenz VSYNC = 15.317626ms == ??? Hz
\item Farbe Pixel = (0,0,1)
\item Farbe Hintergrund = (1,0,1)
\item x-Koordinate = 144
\end{itemize}
